hostname ISP

!

interface GigabitEthernet1/0/1

no switchport

ip address 5.38.152.1 255.255.255.252

ip nat inside

negotiation auto

no shutdown

!

interface GigabitEthernet1/0/2

no switchport

ip address 5.63.195.1 255.255.255.252

ip nat inside

negotiation auto

no shutdown

!

interface GigabitEthernet1/0/3

no switchport

ip address 5.187.135.2 255.255.255.252

ip nat inside

negotiation auto

no shutdown

!

interface GigabitEthernet1/0/4

no switchport

ip address 5.148.200.2 255.255.255.252

ip nat inside

negotiation auto

no shutdown

!

interface GigabitEthernet1/0/5

no switchport

ip address 5.206.190.2 255.255.255.252

ip nat inside

negotiation auto

no shutdown

!

interface GigabitEthernet1/0/36

no switchport

ip address dhcp

ip nat outside

negotiation auto

no shutdown

!

ip nat inside source list 100 interface GigabitEthernet1/0/36 overload

!

ip access-list extended 100

10 permit ip any any

!

end

wr