hostname OFF-FW

!

interface GigabitEthernet1/1

nameif outside

security-level 0

ip address 10.20.255.2 255.255.255.252

!

interface GigabitEthernet1/2

nameif inside

security-level 100

ip address 10.20.254.1 255.255.255.248

!

object network WEBSERVER

host 10.20.254.2

access-list OUTSIDE-IN extended permit tcp any host 10.20.254.2 eq www

access-list OUTSIDE-IN extended permit tcp any host 10.20.254.2 eq https

!

access-group OUTSIDE-IN in interface outside

ip route outside 0.0.0.0 0.0.0.0 10.20.255.1

!

end

wr

#access-group INSIDE-OUT in interface inside

#access-list INSIDE-OUT extended permit ip any an