hostname OFF-L3-2

!

vlan 20

name ACCOUNTING

vlan 21

name SHIPPING

vlan 22

name SALES

vlan 23

name LOGISTICS

vlan 99

name NATIVE

!

ip domain-name ipege.local

crypto key generate rsa modulus 2048

ip ssh version 2

!

username ansible privilege 15 secret ansibleipege

username manage privilege 15 secret management9654

!

int vlan 99

ip address 10.20.99.6 255.255.255.240

no shutdown

!

spanning-tree mode rapid-pvst

spanning-tree vlan 20-21 priority 28672

spanning-tree vlan 22-23,99 priority 24576

!

!

interface range GigabitEthernet1/0/1-5

switchport trunk native vlan 99

switchport trunk allowed vlan 20-23,99

switchport mode trunk

switchport nonegotiate

!

interface range GigabitEthernet1/0/6-34

shutdown

!

interface GigabitEthernet1/0/35

switchport access vlan 99

switchport nonegotiate

!

interface GigabitEthernet1/0/36

switchport access vlan 99

switchport nonegotiate

!

interface range TenGigabitEthernet1/0/37-46

shutdown

!

interface range TenGigabitEthernet1/0/47-48

switchport trunk native vlan 99

switchport trunk allowed vlan 20-23,99

switchport mode trunk

switchport nonegotiate

channel-group 1 mode desirable

spanning-tree link-type point-to-point

!

interface range GigabitEthernet1/1/1-4

shutdown

!

interface range TenGigabitEthernet1/1/1-8

shutdown

!

interface range FortyGigabitEthernet1/1/1-2

shutdown

!

line vty 0 4

transport input ssh

login local

!

end